//---------------------------------------------------------------------------------------
// PC Software Version Info for L-LAS-TB-AL series   
//---------------------------------------------------------------------------------------

	Version:	Date:		Comment:

         -------------------
         V5.0.0  30/Sep/16:   adapt to SI-CON-56F84763-CL V2.0 hardware pcb-board
         V5.0.1  28/Nov/16:   adapt to SI-CON-56F84550-PT V1.0 pardware pcb-board
         V5.0.2  23/Dec/16:   adapt to L-LAS-TB-6-SL (Satisloh)
         V5.0.3  06/Mar/17:   adapt to L-LAS-TB-28-AL
         V5.0.4  23/Mar/17:   adapt to L-LAS-TB-6-AL
         V5.0.5  06/Apr/17:   new EXT-IN0 mode TEACH-PROG with 2 entries
         -------------------
         V5.1.0  10/Oct/17:   data-recorder, scope-function, auto video-thd
         V5.1.1  26/Oct/17:   adapt PROG2/PROG4 behaviour
         V5.1.2  16/Nov/17:   adapt to L-LAS-TB-50-AL and L-LAS-TB-75-AL
         V5.1.3  04/Dez/17:   extend DIG-OUT-MODE to OUT0[-],OUT1[+],OUT2[AL]
                              enlarge arrow-up/down in scope graph,
         -------------------
         V5.2.0  22/Jan/18:   dark-pix-trigger, auto-video-threshold
         V5.2.1  14/Jun/18:   remove update-bug of video-thd after <SEND>

         -------------------
         V5.3.0  08/Apr/19:   new para39: dirt-mode
                              new para40: dirt-threshold
                              new FIX/TRACK/AUTO video-threshold
                              power-mode: STAT, DYN-POW, DYN-ITIME    
         V5.3.1  13/May/19:   remove bug in language-switch and [mm/pix] switch   
	 V5.3.2  09/Dec/19:   adapt to L-LAS-TB-F-6-AL (SL slim-line housing)
	 -------------------

	V5.4.0  02/Mar/20:	Version 5.4.x handles 2-point-linearisation
				and new parameter set for linearisation lookup-table.
				Adapt to L-LAS-TB-F-16-AL-HR (high resolution S124 cmos-line) 

	V5.4.1 26/Mar/20:	Adapt FW 5.4 to L-LAS-TB-28-AL                        
